**Polypropylene filter cartridges**

|  |  |
| --- | --- |
| **Indicators** | **Requirements for regulatory documents** |
| Model | DOE (double sided)  5 µm |
| Material | polypropylene metlblown |
| Overall dimensions:  - length  - external Diametr  - internal diameter | 1016 мм  65 мм  28 мм |
| Degree of purification, throughput | 1-50 microns |
| Operating temperature | 45 оС |
| Working pressure | 8 бар |
| Qty | 1632 pcs |

Flow rate 30m3/hour

  